The probe is capable of piercing through sealants, below is a list of sealants could use.    
  
·        piercing the following materials, at minimum:  
o     Corning Costar Aluminum Sealing Tape (Product #6570)  
o     Excel Scientific AlumaSeal Films for Cold Storage (#FC100)   
  
Please note that the probe could get clogged and maintenance procedures would need to added to the protocol (for instance add wash/rinse command after every 4-5 wells or as needed).